registerity setting for RS232

[HKEY_LOCAL_MACHINE\HARDWARE\DEVICEMAP\TOUCH]
"DriverName"="Touchp.dll"
"CalibrationData"="102,102 1945,102 1945,1945 102,1945"
"COMM"="COM1:"
"BCLEFT"=dword:64
"BCRIGHT"=dword:64
"BCTOP"=dword:64
"BCBOTTOM"=dword:64